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TANGO 750 FRAMING
PR-6630

The user manual contains important information about the safe installation and use of a projector. Please read and follow these instructions carefully and keep the manual in a safe place for future reference.




PR LIGHTING LTD.
http://www.pr-lighting.com
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The following items are supplied with a projector and please check:

	Name
	Quantity
	Unit
	Remark

	Safety cord
	1
	Pc
	

	User manual
	0
	Pc
	QR code 





Please note that as part of our ongoing commitment to continuous product development, specifications are subject to change without notice. Whilst every care is taken in the preparation of the manual we reserve the right to change specifications in the course of product improvement. The publishers cannot be held responsible for the accuracy of the information herein, or any consequence arising from them.
Every unit is tested completely and packed properly by the manufacturer. Please make sure the packing and / or the unit are in good condition before installation and use. Should there be any damage caused by transportation, consult your dealer and do not use the unit. Any damage caused by improper use will not be assumed by the manufacturer and / or dealer.
Note: For the products made by Guangzhou PR lighting Ltd, the warranty for the whole product is one year starting from the delivery date but the light source is not within the warranty.



1. SAFETY AND WARNINGS
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NOTE
Before a projector’s installation, power-on, operation and maintenance, please carefully read 
the safety information hereinafter!



The following safety signs are used in the user manual.
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	[image: 注意安全.jpg]
	● When unpacking , check if there is any damage caused by transportation before using a projector. Should there be any damage, consult your dealer and do not use it.
●The manufacture is not responsible for any loss caused by a user not following the manual or changing a projector as he/she likes. 
●Please be noted that any damage caused by changing the projector at will is not warranted.
● Do not hesitate to contact the dealer or the manufacturer if any questions or advice.
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	● The projector rated for IP66. 
● The projector can be used in damp, over-heat and over-dusty places.
●A projector should be kept away from high temperature, fire, electrical surge, vibration and strong light while being operated.  
●A projector is only intended for installation, operation and maintenance by a qualified person. And the   operation must strictly follow the procedures in the manual. 
●A projector is not for a user to make any replacements and the user shouldn't open a projector for repair and maintenance.


	[image: 防护眼镜.jpg]
	●Don’t look straightly into the light sources especially for epileptics, otherwise eyes will be burned.. 
●Do not connect this device to any type of dimmer pack.
●If the light source, lens and screen protective cover of the a projector have obvious damage, i.e., to the extent that it hurts the performance like cracking or deformation, please stop using it and replace them with the original parts, otherwise its performance will be compromised.
● For the location of a projector, it shouldn’t be seen in the distance of less than 4 meters.
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	●Before operation, please confirm that all covers(housing) are on and screws tightened. It’s forbidden to use a projector while its covers(housing)are off .
●Keep the light source clean and do not touch it with bare hands.
●While operating it, wear protective items like goggle and gloves.
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	●Any electrical connection must be carried out by a qualified person . 
●Before installation, please confirm the voltage supplied matches what is required for a projector.
●Each projector must be properly earthed and installed as per related electrical standards.
●Do not use power cord with its insulator damaged and connect the power cord with other cables.
●If a projector is not used or under cleaning,, please hold its plug and unplug it. Do not unplug it forcefully or by pulling the power cable.
●All power cords must conform to related safety and regulations.
●While being operated, if a projector is not waterproof and dust-proof, it should not be under rains or in humidity to avoid being short. 
●Do not switch on and off a projector constantly in very short intervals, otherwise its light source’s and other electrical parts’  life will be shortened .
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	●There are safety cord holes at the bottom of the base of a projector. In view of safety, please run the safety cord supplied through the safety cord holes for safety support.
●Before any installation, maintenance and cleaning work, please ensure a projector is disconnected from power mains.
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	●While being in stable working state under normal ambient temperature, the temperature of the surface of the metallic housing of a projector including heat sink will reach 75℃.
●While its lamp is stricken for the first time, there will be smoke and strange smell. It’s normal and does not mean a projector has some defects.
●While a projector running, do not touch the metallic housing to avoid being burned.
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	●Do not mount a projector directly on inflammable surface. 
●Do not project the beam straightly on combustible items and the minimum distance between it               
and illuminated items is 10m.
●A projector should be installed with good ventilation and the minimum distance between it and walls is 50cm. At the same time, please ensure the fans and air inlets and outlets are workable.
●Do not let the front lens expose to sunlight or other strong light sources at any angle, otherwise the focused beam inside can result in fire potentially.



[image: ]● The product meets The General Technical Requirements and Standards for Recycle and Use Of 
Expired Appliance and Electronic Products.
● When the product meets disposal standards and needs to be disposed, a client needs to dispose and recycle it.


2. INSTRUCTIONS  
●CLEANING AND MAINTENANCE  
   The accumulation of oil, smoke and dust on the lens will compromise the light output. Cleaning a projector is very necessary to ensure a reliable use of it. The projector is rated for IP66. Unless confirmed by a professional technician for some internal component replacement, it’s forbidden to dismantle a projector.

    Cleaning frequency is to be decided by operations and its environment. Use soft cloth and normal detergent for glass for cleaning work. It’s advised external optical system be cleaned every 20days. Keep lens clean and do not touch optical parts with bare hands.

SPECIAL NOTE    
   
While water-proof projectors are in use,  it’s normal there will be some minor mist on the front lens.
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	●Before any maintenance and cleaning, please ensure a project is off the power.
●Only a qualified person is allowed to do maintenance.
●During maintenance and before maintenance, a projector must be off power.
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	●To avoid sunlight or other light penetrating into the head via the front lens, resulting in high temperature internally causing damages to a projector. Before power-off, please use Tilt channel to move the head and make it facing downward.  
●  Do not use alcohol or other organic solvent to clean the housing to avoid damage.
●  Do not use any solvent with chemical elements to clean color filters or hot mirror.




   
        
●TROUBLESHOOTING
	PROBLEM
	ACTION

	A projector can’t be switched on
	· Check if the fuse is burned 
· Check if the power cord is connected well
· Check if the switching power supply is bad or not connected well. A professional technician is required for the repair
· Check if the control board is connected well. .A professional technician is required for the repair

	A projector can be switched on , but the LED lamp’s brightness can’t be controlled
	· Check if the LED driver board is connected well. A professional technician is required for the repair

	A projector can be switched on normally, but not controlled by the DMX controller 
	· Make sure that its start address is right
· Replace or repair the XLR signal cable.

	The beam is not bright and its brightness decreases sharply
	· Make sure the fans are working well or fans and their shields are not blocked by dust.
· Make sure that the internal optics are clean.

	A project image appears to have a halo
	· Carefully clean the LED lamp, optical lenses and other components.

	Heavily Defective Beam
	· Check if  lens are in good condition(not cracked)
· Clean dust or grease on the lens.




3. INSTALLATION 
●PLACED ON A FLAT SURFACE 

 While placing a projector on a flat surface, tighten the head after loosening its screw and adjusting its angle till desired. For the version with wireless control, while it is on a flat surface its antenna should face upward.


[image: ] (
NOTE
It’s advised to use hexagon screws coupled with anti-slipping washers to ensure firm installation. Whatever screws may be used, they should not be less than 2 pairs.
)

The size of the screws are to be decided by the customer based on the size of mounting holes in the arms, the following sizes in the table are only for reference.
        
	NO
	NAME
	SIZE 
	QTY
	REMARKS

	1
	Hexagon screws
	M12
	4
	Prepared by the customer

	2
	Washer 
	Coupled with the screws 
	4
	Prepared by the customer











         
[bookmark: OLE_LINK5][bookmark: OLE_LINK6]●  POWER CONNECTION

  Connect the power cord as follows:
   L (live) =brown
   E (earth) =yellow/green
   N (neutral) =blue

Before power connection, please ensure the power supplied must match what the nameplate says. It is recommended that each projector be connected with power separately so that they may be individually switched on and off.
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●The earth wire(yellow/green) must be connected to the ground. And electrical connection must be in accordance with the standards concerned.
●If any questions about the electrical installation, do not continue but consult a qualified electrician.
                          ●A projector uses naked wires. For wiring please use waterproof junction box with IP class not lower than IP66.


● THE WIRING OF CONTROL SIGNAL

The colors of signal wires responds to their respective functions:
Blue color –A+
White color –B-
Black color –Shield wire

The shielded 2-core wire between a projector and a controller or between projectors should be not less than 0.5mm in diameter and the maximum number of projectors in a DMX chain should be less than 32 pieces.
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●DMX TERMINATOR 

In the Controller mode, at the last fixture in the chain, its female DMX output has to be connected with a DMX terminator. 
The DMX terminator is simply a Canon connector with a 120 (ohm) resistor connected across pin A+ and pin B-, which prevents electrical noise from disturbing and corrupting the DMX control signals. Before DMX terminator connection, please make proper insulation and waterproof treatment. 
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[bookmark: OLE_LINK7][bookmark: OLE_LINK8]●GOBO FILTER REPLACEMENT


Lock the tilt and loosen the 4 fast-fit screws on the upper cover ,After removing the cover, you will see the structures as the figure above.
To replace a gobo on the rotating gobo wheel: take the rotator from the wheel in the sequence of 1→2 , take the gobo out from the rotator by removing the tightening spring. Put the new gobo back to the rotator, then tighten it with the spring. Please ensure the spring is in the narrow location of the rotator, which is the internal ring of it and flatten it. At last, pull up the spring strip using proper tool and put the rotator back to the wheel with the assistance by another hand. Its installation is of the opposite sequence of removal(（2→1）.
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        Installation of gobos        
                  
NOTE: Do not touch the glass gobo with bare hand. Place clean and soft paper or cloth between hand and glass gobos. 
Tighten 4 hexagon screws after the cover is on. Unlock the tilt.


●FIXING THE FRAMING MODULE 
 (
Note: Please put the plug into the hole for tightening screw for the wheel after unplugging it.
)
 (
Tightening screw for module rotation
) (
Plug
)[image: ]                   [image: ]  


 
Remove the small cover after locking Tilt after adjusting the framing blades. Unplug the plug on the left after tightening the screw against the module till it can’t move . At last, install the small cover.

If the framing blades need to be adjusted, plug the plug into its original place after loosening the tightening screw, then repeat Step 1. 
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        DANGER!

BEFORE REPLACEMENT OF GOBOS/COLOR FILTERS, A PROJECTOR MUST BE OFF THE POWER!





4. SETUP AND CONFIGURATION 

[bookmark: OLE_LINK30][bookmark: OLE_LINK31]●FRONT PANEL OPERATION
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A projector’s configuration can be set conveniently via push button and LCD display. 
Launch the projector and press button ENTER for more than 5 seconds to unlock the panel, the LCD will show the function menu of the projector, each main menu has its submenus and each submenu has a specific function. For details, please see the “OPERATION MENU” section.
To set up or browse through its functions, press button UP or DOWN 
Press button ENTER to save your settings or enter the submenu. 
[bookmark: OLE_LINK71][bookmark: OLE_LINK72]Press button UP or DOWN to change values(plus or minus)
Press button FUNC, it will return to the upper menu. If button FUNC not pressed, the default will show display status automatically.

● DMX START ADDRESS
Each unit must be given a DMX start address so that the correct projector responds to the correct control signals. This DMX start address is the channel number from which the projector starts to “listen” to the digital control information being sent out from the controller. The unit has 3 DMX modes. There are standard mode ,short mode and extended mode. For example standard mode has 30channels, so set the No. 1 projector’s address 001, No. 2 projector’s address 031, No. 3 projector’s address 061, No. 4 projector’s address091, and so on.
Launch the projector. Press button ENTER more than 5seconds to unlock panel.
Press button ENTER to display DMX address; 
Press button UP and DOWN, you can set the address;
Press button ENTER to confirm; after powered on next time, the default will be last value saved
Press button FUNC, it will return to the upper menu
.
●DMX WIRELESS CONTROL (If the projector has the function)
 The projector has wireless control function with wireless receiver module and antenna for remote control.
 The setup of it is below:
1. Enter into the projector’s menu. Select  the menu “Config Settigns” via the bottoms of  UP and DOWN
2. Select DMX control Mode---- Wireless First (Note: do not select XLR ONLY),then wireless indication in the front panel will be on, meaning wireless control function is activated.
Only after the projector is linked with a transmitter, can it receive wireless signal sent by the transmitter. If unlinking it, Press “Enter” for the menu of Unlink Wireless under the upper level menu of Config Settigns .

●STAND-ALONE MODE 
Operate the projector without connecting with a controller, enable the master mode through the operation panel, the projector will run in Stand-Alone mode automatically. 
DMX address can be set at any number within 512.

●MASTER/SLAVE MODE  
Many projectors can run synchronously in the Master/Slave mode by linking them with each other. First,
connect the first fixture’s DMX output to the second fixture’s DMX input using XLR-XLR control cable and then connect the second fixture’s DMX output to the third fixture’s DMX input, and so on until all projector are connected in this way. Eventually connect the last fixture’s DMX output to a DMX terminator. Set 1st  projector as the master and others are Slaves. It’s advised that the maximum quantity of projectors in a DMX chain is less than 32.

Start Addresses of all Slaves are 001; Operation mode of the Master can be set any mode for a Master’ and Slaves’ operation mode can be set accordingly.

After Powered on, the group will run in Master/Slave Mode.( The number of projectors in a DMX chain is 32pcs at maximum)
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5. OPERATION MENU

	1st LEVEL
	2nd LEVEL
	3rd LEVEL
	[bookmark: OLE_LINK20]4th LEVEL
	5th LEVEL

	DMX setting
	DMX Address
	Short Mode:1-486
     Standard Mode:1-483
Extended Mode:1-468
	
	

	Reset
	Total Reset
	Really Reset?
	Confirm/Cancel
	

	
	Colour System Reset
	Really Reset?
	Confirm/Cancel
	

	
	Gobo Reset
	Really Reset?
	Confirm/Cancel
	

	
	Zo.Fo. Fr.Pr. Reset
	Really Reset?
	Confirm/Cancel
	

	
	Other Reset
	Really Reset?
	Confirm/Cancel
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Config Settings

	DMX Channel Mode

	Short Mode 27CH
	
	

	
	
	Standard Mode 30CH
	
	

	
	
	Extended Mode 45CH
	
	

	
	
	View Mode
	001 Strobe
…
	

	
	Signal Select
	XLR Only
	
	

	
	
	XLR First
	
	

	
	
	Wireless Only
	
	

	
	
	Wireless First
	
	

	
	
	Wireless In/XLR Out
	
	

	
	Loss of DMX
	Normal time out
	
	

	
	
	Hold Last Value
	
	

	
	
	White Light
	
	

	
	
	User Memory 1
	
	

	
	
	User Memory 2
	
	

	
	Display Config

	Display Mode
	Off After Delay
	


	
	
	
	On Always
	


	
	
	Display Invert
	Invert OFF
	


	
	
	
	Invert ON
	


	
	
	Language Settings 
	English

	

	
	
	
	Chinese

	

	
	Temperature Unit
	Celsius Degree
	
	

	
	
	Fahrenheit Degree
	
	

	
	Un-Link Wireless
	Really Un-Link?
	Confirm/Cancel
	

	
	Factory Defaults
	Restore Defaults?
	Confirm/Cancel
	

	[bookmark: OLE_LINK56][bookmark: OLE_LINK53]Option Settings 

	Invert Settings 
	Dimmer Invert
	OFF/ ON
	

	
	
	Zoom Invert
	OFF/ ON
	

	
	
	CYM Invert
	OFF/ ON
	

	
	
	CTO Invert
	OFF/ ON
	

	
	Dimmer Settings
	
Gamma Curve
	Gamma 2.0/2.2/2.4/2.6
	

	
	
	
LED Ref. Rate
	1200/2400/4800/10000/12000/15000/20000/25000Hz
	

	
	
	Dimmer Speed
	Fast/Medium/Slow Speed
	

	
	Fan Settings 
	Standard/Theatre
	
	

	
	Blade Detect
	OFF/ ON
	
	

	
	Defaults
	Restore Defaults?
	Confirm/Cancel
	

	[bookmark: OLE_LINK35][bookmark: OLE_LINK33][bookmark: OLE_LINK34][bookmark: _Hlk463775770]Information

	View DMX Values
	
	
	


	
	Total Hours
	Reset Total Hours
	
	

	
	Temperature
	Display Board XX℃/F
	
	

	
	
	Driver Board 1 XX℃/F
	
	

	
	
	Driver Board 2 XX℃/F
	
	

	
	
	Driver Board 3 XX℃/F
	
	

	
	
	Fan Board XX℃/F
	
	

	
	
	LED Sensor XX℃/F
	
	

	
	Software Version
	Display Board
	System= XXX
Boot =XXX
	

	
	
	Driver Board 1
	System= XXX
Boot =XXX
	

	
	
	Driver Board 2 
	System= XXX
Boot =XXX 
	

	
	
	Driver Board 3 
	System= XXX
Boot =XXX
	

	
	
	Fan Board   
	  System= XXX
Boot =XXX
	

	
	Electronic SN
	Electronic SN=
************
	
	

	
	RDM Device Label
	RDM Device Label
ANSI E1.20 RDM
	
	

	
	Fan Status
	Head Fan 
	
	

	Service
	Manual Effect Control
	Strobe                XXX
Dimmer              XXX
……..
	
	



	
	Factory Test
	
	
	

	Operation Mode
	DMX Mode
	Change Operation Mode?
	[bookmark: OLE_LINK65][bookmark: OLE_LINK66]Confirm/Cancel
	

	
	Master Mode
	Preset Memory
	Change Operation Mode?
	Confirm/Cancel

	
	
	User Memory 1
	Change Operation Mode?
	

	
	
	User Memory 2
	Change Operation Mode?
	

	
	Stand-Alone Mode
	Preset Memory
	Change Operation Mode?
	

	
	
	User Memory 1
	Change Operation Mode?
	

	
	
	User Memory 2
	Change Operation Mode?
	

	
	Static Scene
	 Change Operation Mode?
	
	

	[bookmark: OLE_LINK18][bookmark: OLE_LINK19][bookmark: _Hlk463774081][bookmark: OLE_LINK25][bookmark: OLE_LINK26][bookmark: OLE_LINK27][bookmark: _Hlk463775330]User  Memories
	Edit User Memory
	Edit User Memory 1
/Edit User Memory 2
	Scene XX
（1~200Scenes）
	Strobe                XXX
Dimmer              XXX
…….
Delay unit          (msec/s/m)
Link to Step             XXX

	[bookmark: OLE_LINK23][bookmark: _Hlk463775298]
	
	Edit Static Scene
	Strobe              XXX
Dimmer            XXX
…..
	

	[bookmark: OLE_LINK44][bookmark: OLE_LINK45][bookmark: OLE_LINK46][bookmark: _Hlk463782007]
	Init User Memory
	[bookmark: OLE_LINK47]Reset User Memory 1
	[bookmark: OLE_LINK48]Reset User Memory?
	Input Password123

	
	
	Reset User Memory 2
	Reset User Memory?
	Input Password123

	
	
	[bookmark: OLE_LINK50]Reset Static Scene
	Reset Static Scene?
	Input Password123




6. DMX PROTOCOL 

	Short mode
	Standard mode 
	Extended mode 
	Description 
	Decimal low 
	Decimal High 

	1
	1
	1
	Strobe 
	
	

	
	
	
	Close
	0
	

	
	
	
	Pulse strobe from slow to fast 
	1
	127

	
	
	
	Strobe from slow to fast 
	128
	225

	2
	2
	2
	Dimmer 
	
	

	
	
	
	Close
	0
	0

	
	
	
	Linear dimmer (0-100%)
	1
	255

	　
	3
	3
	[bookmark: OLE_LINK1][bookmark: OLE_LINK9]Dimmer in 16 bit 
	
	

	
	
	
	Dimmer in 16 bit adjustment 
	0
	255

	3
	4
	4
	CYM macros 
	
	

	　
	　
	　
	The following functions will disable CMY,CTO, color wheel
	
	

	
	
	
	No function 
	0
	7

	
	
	
	[bookmark: OLE_LINK85][bookmark: OLE_LINK86]Color macro1
	8
	9

	
	
	
	Color macro2
	10
	11

	
	
	
	[bookmark: OLE_LINK87][bookmark: OLE_LINK88]Color macro3
	12
	13

	[bookmark: OLE_LINK89][bookmark: OLE_LINK90]　
	　
	　
	Color macro4
	14
	15

	　
	　
	　
	Color macro5
	16
	17

	　
	　
	　
	Color macro6
	18
	19

	　
	　
	　
	Color macro7
	20
	21

	　
	　
	　
	Color macro8
	22
	23

	
	
	
	Color macro9
	24
	25

	
	
	
	Color macro10
	26
	27

	　
	　
	　
	Color macro11
	28
	29

	
	
	
	Color macro12
	30
	31

	
	
	
	Color macro13
	32
	33

	
	
	
	Color macro14
	34
	35

	
	
	
	Color macro15
	36
	37

	
	
	
	Color macro16
	38
	39

	
	
	
	Color macro17
	40
	41

	
	
	
	Color macro18
	42
	43

	
	
	
	Color macro19
	44
	45

	
	
	
	Color macro20
	46
	47

	
	
	
	Color macro21
	48
	49

	
	
	
	Color macro22
	50
	51

	
	
	
	Color macro23
	52
	53

	
	
	
	Color macro24
	54
	55

	
	
	
	Color macro25
	56
	57

	
	
	
	Color macro26
	58
	59

	
	
	
	Color macro27
	60
	61

	
	
	
	Color macro28
	62
	63

	
	
	
	Color macro29
	64
	65

	
	
	
	Color macro30
	66
	67

	
	
	
	Color macro31
	68
	69

	
	
	
	Color macro32
	70
	71

	
	
	
	Color macro33
	72
	73

	
	
	
	Color macro34
	74
	75

	
	
	
	Color macro35
	76
	77

	
	
	
	Color macro36
	78
	79

	
	
	
	Color macro37
	80
	81

	
	
	
	Color macro38
	82
	83

	
	
	
	Color macro39
	84
	85

	
	
	
	Color macro40
	86
	87

	
	
	
	Color macro41
	88
	89

	
	
	
	Color macro42
	90
	91

	
	
	
	Color macro43
	92
	93

	
	
	
	Color macro44
	94
	95

	
	
	
	Color macro45
	96
	97

	
	
	
	Color macro46
	98
	99

	
	
	
	Color macro47
	100
	101

	
	
	
	Color macro48
	102
	103

	
	
	
	Color macro49
	104
	105

	
	
	
	Color macro50
	106
	107

	
	
	
	Color macro51
	108
	109

	
	
	
	Color macro52
	110
	111

	
	
	
	Color macro53
	112
	113

	
	
	
	Color macro54
	114
	115

	
	
	
	Color macro55
	116
	117

	
	
	
	Color macro56
	118
	119

	
	
	
	Color macro57
	120
	121

	
	
	
	Color macro58
	122
	123

	
	
	
	Color macro59
	124
	125

	
	
	
	Color macro60
	126
	127

	
	
	
	Color macro61
	128
	129

	
	
	
	Color macro62
	130
	131

	
	
	
	Color macro63
	132
	133

	
	
	
	Color macro64
	134
	135

	
	
	
	Color macro65
	136
	137

	
	
	
	Color macro66
	138
	139

	
	
	
	Color macro67
	140
	141

	
	
	
	Color macro68
	142
	143

	
	
	
	Color macro69
	144
	145

	
	
	
	Color macro70
	146
	147

	
	
	
	Color macro71
	148
	149

	
	
	
	Color macro72
	150
	151

	
	
	
	Color macro73
	152
	153

	
	
	
	Color macro74
	154
	155

	
	
	
	Color macro75
	156
	157

	
	
	
	Color macro76
	158
	159

	
	
	
	Color macro77
	160
	161

	
	
	
	Color macro78
	162
	163

	
	
	
	Color macro79
	164
	165

	
	
	
	Color macro80
	166
	167

	
	
	
	Color macro81
	168
	169

	
	
	
	Color macro82
	170
	171

	
	
	
	Color macro83
	172
	173

	
	
	
	Color macro84
	174
	175

	
	
	
	Color macro85
	176
	177

	
	
	
	Color macro86
	178
	179

	
	
	
	Color macro87
	180
	181

	
	
	
	Color macro88
	182
	183

	
	
	
	Color macro89
	184
	185

	
	
	
	Color macro90
	186
	187

	
	
	
	Color macro91
	188
	189

	
	
	
	Color macro92
	190
	191

	
	
	
	Color macro93
	192
	193

	
	
	
	Color macro94
	194
	195

	
	
	
	Color macro95
	196
	197

	
	
	
	Color macro96
	198
	199

	
	
	
	CMY color mixing fade from slow toast 
	200
	255

	4
	5
	5
	Cyan
	
	

	
	
	
	Cyan (Linear  0-100%)
	0
	255

	　
	　
	6
	Cyan in 16 bit 
	
	

	
	
	
	Cyan 16 bit adjustment 
	0
	255

	5
	6
	7
	Yellow 
	
	

	
	
	
	Yellow (Linear 0-100%)
	0
	255

	　
	　
	8
	Yellow in 16 bit 
	
	

	
	
	
	Yellow 16bit adjustment 
	0
	255

	6
	7
	9
	Magenta
	
	

	
	
	
	Magenta (Linear 0-100%)
	0
	255

	　
	　
	10
	Magenta in 16bit 
	
	

	
	
	
	Magenta 16 bit adjustment 
	0
	255

	7
	8
	11
	CTO
	
	

	
	
	
	Linear CTO from high t low
	0
	255

	　
	　
	12
	CTO in 16 bit 
	
	

	
	
	
	CTO 16 bit adjustment 
	0
	255

	8
	9
	13
	Color wheel
	
	

	
	
	
	Continuous positioning 
	
	

	
	
	
	Indexing 0-360°
	0
	63

	
	
	
	Positioning 
	
	

	
	
	
	Open /Color1 
	64
	67

	
	
	
	Color 1
	68
	71

	
	
	
	Color1/Color2
	72
	75

	
	
	
	Color2
	76
	79

	
	
	
	Color2/Color3
	80
	83

	
	
	
	Color3
	84
	87

	
	
	
	Color3/Color4
	88
	91

	
	
	
	Color4
	92
	95

	
	
	
	Color4/Color5
	96
	99

	
	
	
	Color5
	100
	103

	
	
	
	Color5/Color6
	104
	107

	
	
	
	Color6
	108
	111

	
	
	
	Color6 /Color7
	112
	115

	
	
	
	Color7
	116
	119

	
	
	
	Color7 /Open
	120
	123

	
	
	
	Open
	124
	127

	
	
	
	Clockwise rainbow effect from slow to fast 
	128
	191

	
	
	
	Anti-clockwise rainbow effect from slow to fast
	192
	255

	　
	10
	14
	Color wheel in 16bit 
	
	

	
	
	
	Color wheel continuous positioning ,16bit adjustment 
	0
	255

	9
	11
	15
	Rotating gobo wheel 
	
	

	
	
	
	Open
	0
	15

	
	
	
	Gobo1
	16
	29

	
	
	
	Gobo2
	30
	43

	
	
	
	Gobo3
	44
	57

	
	
	
	Gobo4
	58
	71

	
	
	
	Gobo5
	72
	85

	
	
	
	Gobo6
	86
	99

	
	
	
	Gobo7
	100
	113

	
	
	
	Gobo8
	114
	127

	
	
	
	Clockwise rotation from slow to fast 
	128
	147

	
	
	
	Anti-clockwise rotation from slow to fast 
	148
	167

	
	
	
	Gobo1 shakes from slow to fast 
	168
	178

	
	
	
	Gobo2 shakes from slow to fast 
	179
	189

	
	
	
	Gobo3 shakes from slow to fast 
	190
	200

	
	
	
	Gobo4shakes from slow to fast 
	201
	211

	
	
	
	Gobo5shakes from slow to fast 
	212
	222

	
	
	
	Gobo6shakes from slow to fast 
	223
	233

	
	
	
	Gobo7shakes from slow to fast 
	234
	244

	
	
	
	Gobo8shakes from slow to fast 
	245
	255

	10
	12
	16
	Gobo rotation 
	
	

	
	
	
	Indexing  0-360°
	0
	128

	
	
	
	Clockwise rotation from slow to fast 
	129
	188

	
	
	
	Stop
	189
	195

	
	
	
	Anti-clockwise rotation from slow to fast 
	196
	255

	
	13
	17
	Gobo rotation  in 16bit 
	
	

	
	
	
	Gobo rotation 16 bit adjustment 
	0
	255

	11
	14
	18
	Framing blade 1left 
	　
	　

	
	
	
	Linear Framing Blade1 Left Change 0%-100%
	0
	255

	
	
	19
	Framing Blade 1 Left change in 16 bit 
	　
	　

	
	
	
	Framing Blade 1 Left change in 16 bit precision 
	0
	255

	12
	15
	20
	Framing Blade 1 right
	　
	　

	
	
	
	Linear Framing Blade1  Right Change 0%-100%
	0
	255

	
	
	21
	Framing Blade 1 right change in 16 bit 
	　
	　

	
	
	
	Framing Blade 1 right change in 16 bit precision 
	0
	255

	13
	16
	22
	Framing Blade 2 Left
	　
	　

	
	
	
	Linear Framing Blade2 Left Change 0%-100%
	0
	255

	
	
	23
	Framing Blade 2 Left change in 16 bit 
	　
	　

	
	
	
	Framing Blade 2 Left change in 16 bit precision 
	0
	255

	14
	17
	24
	Framing Blade 2 Right
	　
	　

	
	
	
	Linear Framing Blade2 Right Change 0%-100%
	0
	255

	　
	　
	25
	Framing Blade 2 right change in 16 bit 
	　
	　

	
	
	
	Framing Blade 2 right change in 16 bit precision 
	0
	255

	15
	18
	26
	Framing Blade 3 Left
	　
	　

	
	
	
	Linear Framing Blade3 Left Change 0%-100%
	0
	255

	
	
	27
	Framing Blade 3 Left change in 16 bit 
	　
	　

	
	
	
	Framing Blade 3Left change in 16 bit precision 
	0
	255

	16
	19
	28
	Framing Blade 3 Right
	　
	　

	
	
	
	Linear Framing Blade3 Right Change 0%-100%
	0
	255

	
	
	29
	Framing Blade 3 right change in 16 bit 
	　
	　

	
	
	
	Framing Blade 3right change in 16 bit precision 
	0
	255

	17
	20
	30
	Framing Blade 4 Left
	　
	　

	
	
	
	Linear Framing Blade4Left Change 0%-100%
	0
	255

	
	
	31
	Framing Blade 4 Left change in 16 bit 
	　
	　

	
	
	
	Framing Blade 4Left change in 16 bit precision 
	0
	255

	18
	21
	32
	Framing Blade 4 Right
	　
	　

	
	
	
	Linear Framing Blade4Right Change 0%-100%
	0
	255

	
	
	33
	Framing Blade 4 right change in 16 bit 
	　
	　

	
	
	
	Framing Blade 4right change in 16 bit precision 
	0
	255

	19
	22
	34
	Framing Module rotation
	
	

	
	
	
	Framing Module  Indexing(0-90degrees)
	0
	255

	
	
	35
	Framing Module rotation in 16 bit
	
	

	
	
	
	Framing Module rotation(0-90degrees) in 16 bit 
	0
	255

	20
	23
	36
	Prism 
	
	

	
	
	
	No
	0
	16

	
	
	
	Prism in 
	17
	255

	21
	24
	37
	Prism rotation 
	
	

	
	
	
	Prism indexing 
	0
	127

	
	
	
	Stop
	128
	

	
	
	
	Clockwise rotation from slow to fast
	129
	191

	
	
	
	Stop
	192
	

	
	
	
	Anti-clockwise rotation from slow to fast 
	193
	255

	22
	25
	38
	Effect wheel 
	
	

	
	
	
	No 
	0
	19

	
	
	
	Effect wheel in 
	20
	255

	23
	26
	39
	Effect wheel rotation 
	
	

	
	
	
	Clockwise rotation from fast to slow
	0
	127

	
	
	
	Anti-clockwise rotation from slow to fast 
	128
	255

	24
	27
	40
	Frost 
	
	

	
	
	
	Linear frost 0% - 100%
	0
	255

	25
	28
	41
	Focus 
	
	

	
	
	
	Linear focus 
	0
	255

	
	
	42
	Focus in 16 bit 
	
	

	
	
	
	Focus 16 bit adjustment 
	0
	255

	26
	29
	43
	Zoom 
	
	

	
	
	
	Linear Zoom 
	0
	255

	
	
	44
	Zoom in 16 bit 
	
	

	
	
	
	Zoom 16 bit adjustment 
	0
	255

	[bookmark: _GoBack]27
	30
	45
	Power/Special function 
	
	

	
	
	
	No function 
	0
	4

	
	
	
	Reserved 
	5
	19

	
	
	
	The following function must stay in the DMX range for more than 5s to activate it
	
	

	
	
	
	Display on 
	20
	24

	
	
	
	Display off
	25
	29

	
	
	
	Reserved 
	30
	44

	
	
	
	Reserved 
	45
	46

	
	
	
	Fan standard mode 
	47
	48

	
	
	
	Fan theater mode 
	49
	50

	
	
	
	Reserved 
	51
	52

	
	
	
	Fast dimmer speed 
	53
	54

	
	
	
	Medium dimmer speed 
	55
	56

	
	
	
	Slow dimmer speed 
	57
	58

	
	
	
	Gamma curve 2.0 
	59
	60

	
	
	
	Gamma curve 2.2
	61
	62

	
	
	
	Gamma curve 2.4
	63
	64

	
	
	
	Gamma curve 2.6
	65
	66

	
	
	
	LED fresh rate 1200Hz
	67
	68

	
	
	
	LED refresh rate 2400Hz
	69
	70

	
	
	
	LED refresh rate 4800Hz
	71
	72

	
	
	
	LED refresh rate 10000Hz
	73
	74

	
	
	
	LED refresh rate 12000Hz
	75
	76

	
	
	
	LED refresh rate 15000Hz
	77
	78

	
	
	
	LED refresh rate 20000Hz
	79
	80

	
	
	
	LED refresh rate 25000Hz
	81
	82

	
	
	
	Reserved
	83
	149

	
	
	
	Color system reset 
	150
	159

	
	
	
	Gobo wheel reset 
	160
	169

	
	
	
	Reserved 
	170
	179

	
	
	
	Zoom/Focus/Frost/Prism reset
	180
	189

	
	
	
	Other（effect wheel, framing module）reset
	190
	199

	
	
	
	Total reset 
	200
	209

	
	
	
	Reserved 
	210
	255



Remarks:
Fan errors can result in LED lamp off automatically
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8. ERROR MESSAGE 
The system can detect some errors during the reset, if [image: 主页-错误警告.png] displayed, press ENTER button to view the error.
The error messages are as follows:

	Name 
	Type
	Correction 

	Cyan 
	Timeout
	Check if wiring, positioning parts and motors are normal

	Yellow 
	Timeout
	Check if wiring, positioning parts and motors are normal

	Magenta 
	Timeout
	Check if wiring, positioning parts and motors are normal

	CTO
	Timeout
	Check if wiring, positioning parts and motors are normal

	Color Wheel 
	Timeout
	Check if wiring, positioning parts and motors are normal

	Rot. Gobo Wheel 
	Timeout
	Check if wiring, positioning parts and motors are normal

	Rot. Gobo Rotation
	Timeout
	Check if wiring, positioning parts and motors are normal

	Dimmer 
	Timeout
	Check if wiring, positioning parts and motors are normal

	Prism 
	Timeout
	Check if wiring, positioning parts and motors are normal

	Prism  Rotation
	Timeout
	Check if wiring, positioning parts and motors are normal

	Focus
	Timeout
	Check if wiring, positioning parts and motors are normal

	Zoom
	Timeout
	Check if wiring, positioning parts and motors are normal

	Effect wheel 
	Timeout
	Check if wiring, positioning parts and motors are normal

	Effect wheel rotation 
	Timeout
	Check if wiring, positioning parts and motors are normal

	Framing module rotation
	Timeout
	Check if wiring, positioning parts and motors are normal

	Driver Board 1
	Error
	Check signal wire

	Driver Board 2
	Error
	Check signal wire

	Driver Board 3 
	Error 
	Check signal wire

	Framing module board 
	Error
	Check signal wire

	Fan Board
	Error
	Check signal wire

	Lamp Off[Fan Error]
	Error 
	Check if all fans are normal

	Time IC
	Error
	



9. TECHNICAL DATA 
	ELECTRIC PARAMETERS   
Input voltage 100V~240V AC，50/60Hz
Input power  750W@220V AC
            790W @ 100V AC
Power factor PF>0.9


	THE SPECIFICATIONS OF THE LIGHT SOURCE
Power                             500W White LED
Color temperature                    9000K
Rated life                           20000hrs 
CRI                               Ra≥70( Option: Ra≥90)
    

	                                                                           
COLORS
[image: ]CMY linear mixing system with macros
1 color wheel: 7exchangeable colors+ Open
Half color effect, rainbow effect with bi-directional and variable speeds,              
Stepping/linear color changing

CTO
0-100% linear CTO

GOBO
1 Rotating Gobo Wheel: 8 replaceable gobos+ Open, Glass or Metal Gobo
Bi-directional Rotation with variable speeds 
With Indexing Function 
Gobo Shake Effect with Variable Speeds 
Bi-directional Scrolling with Variable Speeds 
Gobo outer size:24mm Gobo image size: 18mm
1framing module rotates between 0° and 90° and produces graphics of different shapes and sizes 
4 framing blades can produce full curtain effect 

		[image: ]
	[image: ]
	[image: ]
	[image: ]
	[image: 120150354.jpg]

	1#
	2#
	3#
	4#
	5#

	[image: 120150355.jpg]
	[image: 120150356.jpg]
	[image: 120150357.jpg]
	
	

	6#
	7#
	8#
	
	




	PRISM

	1pc of  3  facet prism , Bi-directional rotation with variable speeds and indexing function

FROST 
1pc frost filter, linear frost effect( 0%-100%)


	EFFECT WHEEL
1pc, replaceable, bi-directional rotation with variable speeds 

FOCUS
DMX linear Focusing 

DIMMER
0-100% Linear adjustment 

	STROBE
Double shutter blades, 0.3~25 F.P.S

TILT
270°

	

	BEAM ANGLE（With Open hole）

	linear zoom  5°～  40° with 16 bit function 


	[bookmark: OLE_LINK32][bookmark: OLE_LINK36]CONTROL

	DMX512, 5 pin interfaces
RDM control protocol 

	27channels in short mode,30channels in standard mode and45channels in extended mode 
Master/Slave synchronized mode
Stand-alone mode

	

	

	OTHER FUNCTION 
Total hours displayable 

	English and Chinese menus
Built-in sensor diagnostic system 
Software versions displayable 
Input signal isolation  

	Modular Structure for easy maintenance

	

	HOUSING
High temperature ABS+ High tensile cast aluminum , IP66

	

	NET WEIGHT
32Kg

	
OPERATION TEMPERATURE
Highest ambient temperature 45℃
Note: If the ambient temperature is below -20°C, reset a projector before pre-heating it for more than 30 minutes 

	
SIZES (unit: mm)

[image: ]

SIZE OF MOUNTING HOLES IN THE BASE (Unit mm) 

[image: ]



LIGHT OUTPUT
[image: ]
10. COMPONENT ORDER CODES 

	NAME 
	CODE NO.
	QTY.
	REMARKS 

	SWITCHING POWER SUPPLY 
	192010228
	1
	

	LED MODULE 
	150020337

	1
	

	LED MODULE FAN 
	030060116
	1
	

	BLOWER FOR GOBO WHEEL 
	030060106
	1
	

	FAN FOR POWER SUPPLY IN THE BASE 
	030060075
	1
	

	LED DRIVER FAN 
	030060084
	1
	

	FAN FOR LENS ACCESSORY 
	030060104
	1
	

	BLOWER FOR LENS ACCESSORY
	030060072A
	1
	

	FOCUS MOTOR 
	030040213A
	1
	

	ZOOM MOTOR 
	030040154A
	1
	

	PRISM IN/OUT MOTOR 
	030040132A
	1
	

	PRISM ROTATION MOTOR
	030040203
	1
	

	FROST MOTOR 
	030040220A
	1
	

	ROTATING GOBO WHEEL MOTOR 
	030040215A
	1
	

	GOBO ROTATION MOTOR 
	030040293
	1
	

	EFFECT WHEEL IN/OUT MOTOR
	030040236
	1
	

	EFFECT WHEEL ROTATION MOTOR 
	030040224C
	1
	

	COLOR WHEEL MOTOR 
	030040154A
	1
	

	CMY MOTOR 
	030040211A
	3
	

	CTO MOTOR 
	030040211A
	1
	





























































































PR LIGHTING LTD.

1582 Xingye Avenue, Nancun Panyu
Guangzhou, 511442 China
TEL: +86-20-3995 2888

PR lighting will try its best to offer accurate and overall information about a product’s technical data. Any changes won’t be notified if necessary. Patented Products. Counterfeiting Will be Prosecuted!
P/N: 320021372
Old Version:20220927
New Version:20221112
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